|  |
| --- |
| Ertuğrul Yolcu  Musa Ulusoy  Ece İrem Yazır 2376101 |
|  |
|  |

|  |
| --- |
| EE464 HARDWARE PROJECT |
| Design Report |
| Formlar ve Görseller | ODTÜ ELEKTRİK - ELEKTRONİK MÜHENDİSLİĞİ |

# Intro

This project is based on the need for an isolated DC-DC converter that takes an input voltage from 24V to 48V and gives a constant output of 15V at 45W with closed-loop control. The chosen converter design’s both lines, and load regulations, as well as the output voltage ripple, needs to be 3%. This design report will focus on the topology and its component selections due to these constraints. Analytical calculations for electrical and magnetic design and overall simulation results will be discussed.

Table 1 Project Constrains

|  |  |
| --- | --- |
| Input Voltage Range | 24-48V |
| Output Voltage | 15V |
| Output Power | 45W |
| Line Regulation Percentage | 3% |
| Load Regulation Percentage | 3% |
| Output P-P Voltage Ripple | 3% |

# Topology Selection

In this project, fundamental flyback topology is chosen. Flyback converters are used mostly in low to medium power applications, so this was the main reason why we tend to choose this topology. Also, this topology is chosen due to its simplicity in construct and control, especially in discontinuous conduction mode. It has a smaller number of circuit elements (mainly passive elements); also, no energy storage inductor is needed because of the transformer, and only one diode is used in the topology, which causes less loss in the system. Also, there are more minor EMI problems with respect to other isolated topologies.




Figure 1 Flyback Converter Topology




Figure 2 Isolated Converter Topologies Comparison (retrieved from Würth Elektronik)

# DESIGN

# CONTROLLER DESIGN

There are different kinds of controllers we have found and implemented in LTspice. The first one is LT3751 which is a capacitor charger. The main advantage of the controller has UVLO/OVLO pins that are used for selecting the input voltage range. Another advantage of the controller is that two resistors which are RVout and RBG, are used to set up the output voltage.




Figure 1 Block diagram of the LT3751

Also, this controller has the ability to operate in DCM operation, which increases the efficiency of the converter, which is really critical for the project. At that point, most of the requirements for the project are satisfied, whereas this controller is used for the capacitor charger, emphasized at the beginning. Because of that, when this controller was used with the load which is 5Ω in this project, the output voltage decreased to zero. In these controller applications, output voltage regulation resistors exist for high output values. On the other hand, we are trying to regulate the voltage at the 15V and 45W output. In this step, we could not reach the required voltage level because of the step size of the controller. The reason behind this is the controller, which is LT3751, is created for high voltage values. The digital voltage step size of the controller is higher than 15V.

After this controller, a lot of different kinds of controllers are implemented in LTspice and Simulink. Unfortunately, most of them could not reach the requirements that are specified in the project description. After the search step, we have found the LT3748, which is created by Linear technology. LT3748 is the isolated flyback converter controller. The advantages of this controller can be listed as:

-Wide input range and controllable lower threshold

-No transformer third winding or opto-isolator required for regulation

-Primary side winding feedback load regulation

-The LT3748 has different kinds of advantages besides those. The regulated output voltage can be decided as with the formula:

-Another advantage of the controller is indicating the inductance limitations which are upper and lower bounds for the transformer design. This part will be explained in the transformer design step.




Figure 2 Block diagram of the LT3748

The manufacturer of this controller which is Analog Devices, has created the LTspice models for this chip. Thanks to that, we have implemented the schematic of the flyback converter with LT3748.

Another chosen controller is LM51561 which is created by Texas Instruments. This controller is the second option for us. The advantages of this controller are wide and controllable input range, controllable output voltage, small size and low cost, and constant peak current limiting over input. The features of the LM51561 is similar to the LT3748. Both of them are ordered and the applications will be started with the LT3748.




Figure 3 Block diagram of the LM56511

Our last option for the controller is using STM32 or Arduino to control the converter. At this point, the controller was designed to change the DON and Doff time.

# SNUBBER DESIGN

The voltage increase at the drain side of the MOSFET, when the switch is off, appearing because of the leakage inductance of the transformer. When the current at the input side is high enough, more stored energy needs to be dissipated. Because of that, leakage inductances of the transformer need to be minimized. Considering the inadequacy or failure of the snubber circuitry, the VDS voltage rating of the MOSFET can be chosen with the safety margin. There are different kinds of snubber circuit designs that exist. One of the popular ones is the RCD snubber circuit. Another one is the Zener snubber circuit. The advantage of the Zener suppressing circuit is dissipating the power when the voltage reaches the dangerous voltage level for the MOSFET.




Figure 4 RCD Snubber circuitry




Figure 5 Snubber Circuit with Zener Diode

The advised approach for designing the snubber circuitry is measuring the period of the ringing when the switch is off without snubber circuitry. After that, the snubber capacitor needs to be added to the circuit starting from the feasible capacitance like 100pF. When the damping period reaches 1.5 -2 times longer, the capacitor is chosen. The change in period can determine the value of the parasitic capacitance, and the initial period of the damping can determine the leakage inductance. In addition to that, those values can be determined from the leakage inductance of the transformer and switch capacitance. When this inductance and capacitance value is determined, the resistance of the snubber needs to be decided.




Figure 6 Effect of the Snubber taken from the Datasheet of the LT3748

Dissipated power will be equal to:

# TRANSFORMER DESIGN

For the transformer design, the start point was the controller’s limitations. According to the chosen IC LT3748, primary inductance has the following limitations:

The gain formula of the flyback converter is So, for the max Vin, D=0.27. For the min Vin, D=0.43. The operating frequency is chosen as 80 kHz. Hence, ton(min)=Dmin/f­sw=3.37 µs.

So .

LPRI is chosen as 55 µH inside these constraints. After this step, the core was chosen by the following step:

.

According to these, the most suitable core was KOOL MU 00K3515E090 since it has the lowest multiplication. Then, turn numbers found with the parameters of this core:

After finding the turns number, by using the RMS values of the primary and secondary side currents, cable selection was made:




Figure 7:Primary side rms current




Figure 8:Secondary side RMS current

According to the simulations, the primary side voltage is a maximum 3.6 A. Secondary side voltage is a maximum 4.8 A. For a safety margin, the primary side current was chosen as 4A, and the secondary side voltage was chosen as 5A.

* For the primary side:
* For the secondary side:

For the cable selection, AWG 26 cable was chosen due to the high operating frequency margin. However, in the lab, there was AWG 25 cable with 0.162 mm2 cross-section area and %100 skin depth at 85 kHz. Hence, we carried on with this cable.

* For the primary side:
* For the secondary side:

After we implemented the cables in the lab, they did not fit into the selected core. In real life, it showed us with these cable selections and turns number, the fill factor must be higher than 1. So, the core selection is changed again.

After we searched the core inventory, the most suitable core was ferrite 0P44022EC core since, due to its material, leakage would be much less than the kool mu core. Also, its cross-section and window area is large enough to fit the cables. Then, all the calculations were made for this core. For the turn number, Al value of the core is important. So, if we change the A­l value of the core by adding an air gap to the core, we can acquire the desired turn numbers.

* Let’s assume the turn numbers as Npri = 12, Nsec = 9.5
* So,

So, by adding this air gap to the core, we can obtain the required reluctance value. If we calculate the magnetic flux density as

Hence, by this calculation, we can see that core is not saturated. It is not the expected value since we did all the calculations for B= 0.2 T. However, this result is close enough to the expected value, and it does not saturate the core. After that, the fill factor is calculated as follows:

It can be deducted that the fill factor is very small, and it shows that the core is overdesigned for this situation. However, since we built the transformer by hand, the fill factor is not high enough.

## IMPLEMENTATION

The transformer was implemented according to calculations. However, as expected, real-life and theoretical calculations did not match exactly. After implementing the transformer, we did the measurements.

A picture containing text, indoor

Description automatically generated

Figure 9:Primary side inductance

For the primary side inductance measurement, which is magnetizing inductance, we left open the secondary side and connected the probes of the LCR meter to the primary side. The result of the measurement can be seen in Fig.11. The expected value was 55 µH, but it was measured as 53 µH. It is very close to the expected value.



Figure 10:Secondary side inductance

For the secondary side inductance measurement, we left open the primary side and connected the probes of the LCR meter to the secondary side. The result of the measurement can be seen in Figure 12. It was measured as 36 µH.

If the turns ratio is checked by the inductance values, the turns ratio can be found as

So, the turns ratio is satisfied by the inductance values.



Figure 11:Leakage inductance value

For the leakage inductance, we shorted the secondary side and connected the probes to the primary side. The connection can be seen in Figure 14. Since it was thought that we might change the turns in the future, excess cables did not cut out. Hence, resulted in more leakage inductance of 2.6 µH, which can be seen in Figure 13.




Figure 12:Leakage inductance measurement

## LOSSES

### Copper Losses

For the copper losses, we need to find how much cable is used. To obtain this information, dimensions of the core must be known

Diagram

Description automatically generated

Figure 13:Dimensions of the core

Dimensions of the core are represented in the figure above. According to this figure,

### Core Loss

According to the core loss per cm3 value of the core, approximate core loss is calculated as follows:

Since we are operating at high frequencies, core losses are much higher than the copper losses, and it is expected.

# COMPONENT CALCULATIONS

## Output Capacitor

From the voltage gain expression of the flyback converter, our duty cycle becomes

= N21 \* where N12 is chosen as 1.23

So, the duty limits become 0.44 for 24V input and 0.28 for 48V input.

= 0.03

D/(0.03\*5\*80kHz) = Co

Co has to be at least 36.7 µF (For 24 V input voltage) from the converter equations.

On the other hand, from the LT3748 datasheet output capacitor can be specified as




Figure 14 Output Voltage Equation with respect to Limiting Current

ILIM = = 8.62A (Duty approximated as 0.37)




Figure 15 Output Capacitor Equation from the LT3748 Datasheet

0.03\*15 =

**Co = 302.72 µF**

## Diode and Switch




Figure 16 Diode RMS Current Equation from the Datasheet

ID(RMS) == 4.86A




Figure 17 Peak Values for Switch





Figure 18 MOSFET RMS Current Equation from the Datasheet

IMOS(RMS) = = 3.03A

Vsw(max) = 48/(1-0.28) = 66.7V

Isw(max) = 3/0.8856+ 5.6 ≈ 9A (where Lm is 4.32µH)

## Feedback and Reference Resistances



Where VBG bandgap voltage for a silicon switch is around 1.2 V,

NPS = N1/N2 = 1.23,

the forward voltage drop of the diode is 1.2V,

Equivalent series resistance on the secondary side is //ωL2//Ro ≈ 0

= 16.6

So, when RREF is given as 6.1kΩ (limited in the datasheet) RFB becomes around 100kΩ.

# SIMULATION RESULTS AND COMPONENT SELECTION




Figure 19 Circuit Diagram for the overall design with LT3748

Due to the above calculations in the previous section, the simulation circuit has been set, as seen in Figure 21.




Figure 20 Diode and Switch Currents for the Transient Part





Figure 21 Diode and Switch Current Maxima




Figure 22 Diode and switch voltages

As seen in Figures 22 and 23, the diode selected must be able to handle at least 12 amperes, and the switch must handle 10 amperes. Also, Figure 24 shows that the switch must endure 60 volts, and the diode must handle at least 55 volts.

For simplicity, the switch is chosen from the lab inventory since the components match with the ratings. IRF540 N-type MOSFET is chosen since it has 100V-27A ratings that can handle our circuit’s needs. For the diode, DS16-01AS-TRL with 100V-16A ratings is chosen.




Figure 23 Output capacitor voltage and current for the transient interval

As obtained in Figure 25, the output voltage sees almost 16 volts in the transient time interval, so the output capacitor must bear this voltage. Also, the current seen by this capacitor reaches almost 11 amperes. After checking the most accessible stocks, the **SD1V337M1012MPA** capacitor has been our choice.This capacitor is 330µF and can handle 35V & 0.63A ripple current.




Figure 24 Output Voltage Ripple

As seen in Fig.26, the output ripple is around 0.15 Volts.





Figure 25 Vout deviation when the input goes from 24V to 48V





Figure 26 Vout deviation when Io changes from 100% to 10%

Line regulation from our simulation can be seen in Fig.27 as (15.19-15.046) \* 100/15.19 = 0.947 % and load regulation can be seen in Figure 28 as (15.111-15.046) \* 100/15.111 = 0.43%.